# Sample Production Plan – iPad/Laptop Bag

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Step** | **Details** | **Time line** | **Class** |
| **1** | Cut fabric | Cut out all fabric. Measure twice cut once! | 90 mins | 1 |
| **2** | Make pockets | Attach pockets to outside or lining (depending on where your pocket is on your design) | 30 mins | 2 |
| **3** | Sew outside | Sew the outside of bag (denim/cotton drill) together on three sides RIGHT SIDES TOGETHER, leaving top side open, trim corners. Turn right way around and iron. | 20 mins | 2 |
| **4** | Sew lining | Sew the lining of bag together on three sides RIGHT SIDES TOGETHER, leaving top side open, trim corners. | 15 mins | 2 |
| **5** | Sew flap | Sew the flap pieces of bag together on three sides RIGHT SIDES TOGETHER, leaving top side open, trim corners. Turn right way around and iron. | 20 mins | 3 |
| **6** | Top stitch flap | Top stitch around the three sewn sides of the flap. | 15 mins | 3 |
| **7** | Prepare strap | Iron the strap lengthways into four even columns | 10 mins | 3 |
| **8** | Sew strap | Top stitch down both sides of the strap | 15 mins | 3 |
| **9** | Baste strap and flap | Baste the strap and flap into position on the outside of the bag. | 15 mins | 4 |
| **10** | Construct bag | Put denim/cotton drill bag, flap and strap right side out) inside the lining (inside out) so that the right sides of the bags are together. Sew around ¾ of the opening – leave a 10cm gap for turning bag right way around. | 30 mins | 4 |
| **11** | Iron bag | Turn bag right way around, and iron – taking care to iron the opening evenly. | 10 mins | 4 |
| **12** | Finish off bag | Top stitch around the mouth of the bag – taking care to sew the opening shut. | 20 mins | 5 |